# UPW: Upstream Weighting package file created on 09/02/2016 by ModelMuse version 3.6.3.0.
 9 -1.000000000000E+020  0 1 # Data Set 1, IUPWCB HDRY NPUPW IPHDRY
 1 1 1 0 # LAYTYP
 0 0 0 0 # LAYAVG
 -1 -1 -1 -1 # CHANI
 0 0 0 0 # LAYVKA
 0 0 0 0 # LAYWET
CONSTANT    1.000000000000E-005  # HK Aluvial Layer 1
CONSTANT    1.000000000000E+000  # HANI Aluvial Layer 1
CONSTANT    1.000000000000E-005  # VKA Aluvial Layer 1
CONSTANT    1.000000000000E-007  # HK UpperFracAq Layer 2
CONSTANT    1.000000000000E+000  # HANI UpperFracAq Layer 2
CONSTANT    1.000000000000E-007  # VKA UpperFracAq Layer 2
CONSTANT    1.000000000000E-008  # HK MiddleFracAq Layer 3
CONSTANT    1.000000000000E+000  # HANI MiddleFracAq Layer 3
CONSTANT    1.000000000000E-008  # VKA MiddleFracAq Layer 3
CONSTANT    1.000000000000E-009  # HK LowerFracAq Layer 4
CONSTANT    1.000000000000E+000  # HANI LowerFracAq Layer 4
CONSTANT    1.000000000000E-009  # VKA LowerFracAq Layer 4
